**Application for Temporary Propane Tank Installation**

**100-2,000 Gallon Capacity**

Installer Information:

|  |  |  |  |
| --- | --- | --- | --- |
| Name of Installer:  |  | Permit Fee:  | $**66.50** |
| Address:  |  | Installation Date: |  |
|   |  | Est. Removal Date: |  |
| Contact Person: |  | Phone: |  |
| Gas Supplier: |  | Phone: |  |

General:

Installation to comply with attached letter, the latest edition of NFPA 58, and with all applicable regulations of the State of Minnesota and the City.

Proposed Installation Site Information:

|  |  |  |  |
| --- | --- | --- | --- |
| Name of Customer: |  | Number of tanks: |  |
| Address of Installation: |  | Size of Tanks: |  |
| Purpose of Installation: |  | Building Type: |  |
| Type of Vaporizer: |  | Tank to vaporizer  |  |

Distances:

|  |  |  |  |
| --- | --- | --- | --- |
| Tank to nearest property line that can be built upon  |  | Tank to building  |  |
| Vaporizer to building  |  | Distance between tanks  |  |

Who is responsible for piping and connections from tank(s) to the building and devices?

|  |
| --- |
|  |
| Remarks: |  |
|  |

 **N**

**W E**

 **S**

 **Building Tank Vaporizer**

TEMPORARY LP USE CONDITIONS

1. **ALL INSTALLATIONS MUST BE IN ACCORDANCE WITH ALL APPLICABLE STATE AND LOCAL ORDINANCES, STANDARDS, AND CODES, INCLUDING MSBC, MSFC, AND NFPA 58.**
2. OBTAIN ALL APPROPRIATE CITY PERMITS.
3. SITE PLAN AND STORAGE SPECIFICATIONS SHALL BE APPROVED PRIOR TO INSTALLATION.
4. ALL PORTABLE TANKS SHALL BE USED AND STORED IN ACCORDANCE WITH ALL APPLICABLE CODES AND REGULATIONS.
5. Containers shall be protected by an approved method. NFPA 58
6. Storage area shall be placed on an approved surface.
7. Storage areas shall be clearly labeled.
8. Storage areas shall be located at least 5’ from any exit or opening. NFPA 58
9. ALL DISTRIBUTION PIPING MUST BE INSTALLED IN ACCORDANCE WITH CITY AND STATE CODES. **HOSE LENGTH SHALL NOT EXCEED 6’ EXCEPT AS APPROVED BY THE FIRE DEPARTMENT.**
10. **NO COMBUSTIBLE PRODUCTS CAN BE STORED NEAR THE TANKS THAT ARE IN USE OR BEING STORED.**
11. VEHICLE PROTECTION MUST BE PROVIDED AND APPROVED.
12. 500 GAL. TANKS SHALL ONLY BE MOVED BY THE SUPPLIER.
13. **INSTALLATION SHALL BE IN ACCORDANCE WITH THE ATTACHED HANDOUT.**
14. APPROVED FIRE EXTINGUISHER MUST BE PRESENT AND READILY AVAILABLE.
15. **PRE-CONNECTION VISIT FROM FIRE DEPARTMENT IS REQUIRED FOR ALL PORTABLE AND STATIONARY TANKS. CALL 651-552-4172 AT LEAST 2 BUSINESS DAYS IN ADVANCE TO SCHEDULE.**