**COMMERCIAL KITCHEN**

**FIRE SUPPRESSION SYSTEM**

**PERMIT APPLICATION**

|  |  |  |  |
| --- | --- | --- | --- |
| APPLICATION DATE: | |  | |
| TYPE OF WORK: |  | | | |
| ESTIMATED DATE OF COMPLETION: | | |  | | |

|  |  |  |  |
| --- | --- | --- | --- |
| **SITE INFORMATION** | | | |
| ADDRESS: | |  | |
| NAME: |  | | |
| OWNER NAME: | | |  |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CONTRACTOR INFORMATION** | | | | | | | |
| COMPANY NAME: | |  | | | |  |  |
| CONTACT: | |  | | | | STATE #: |  |
| ADDRESS: | |  | | | | | |
| STATE/ZIP CODE: | | |  | | | | |
| PHONE #: |  | | | FAX #: |  | | |

FEE SCHEDULE PER CITY ORDINANCE:

Fire Department Permit Fee ------------------------------------------------------- $66.50

All permit applications must be accompanied with:

1. Two complete sets of drawings and specifications.
2. Cut sheets on materials and components to be used.
3. Description of the work to be performed.

The undersigned hereby agrees to complete the project in accordance with the Ordinances of the City, MN State Building Code, MN State Fire Code and to all other recognized codes or standards.

|  |  |
| --- | --- |
| SIGNED: |  |
| PRINTED: |  |

ADDITIONAL CONDITIONS

1. THE INSTALLATION OF THE FIRE SUPPRESSION HOOD SYSTEM MUST BE IN ACCORDANCE WITH APPLICABLE AND RECOGNIZED STANDARDS AND CODES.
2. ANY CHANGES OR VARIATIONS TO THE APPROVED PLAN MUST BE SUBMITTED IN WRITING PRIOR TO WORK BEING CONDUCTED.
3. ALL NECESSARY CITY PERMITS MUST BE APPLIED FOR AND GRANTED PRIOR TO WORK BEING CONDUCTED. (MECHANICAL, ELECTRICAL, PLUMBING, AND BUILDING).
4. ALL APPLIANCES SHALL HAVE CORRECT CLEARANCES UNDER THE HOOD SYSTEM.
5. ALL APPLIANCES UNDER THE HOOD SYSTEM MUST HAVE SHUNTS.
6. **EXHAUST MUST REMAIN ON AFTER ACTIVATION.**
7. EXHAUST/MAKE-UP INTERLOCK SHALL BE INSTALLED PER THE MMC and NFPA 96.
8. PROPER PLACEMENT OF A CLASS K EXTINGUISHER IS REQUIRED BEFORE FINAL INSPECTION.
9. WHERE A BUILDING FIRE ALARM SYSTEM IS INSTALLED, NEWLY INSTALLED AUTOMATIC FIRE EXTINGUISHING SYSTEMS SHALL BE MONITORED BY THE BUILDING FIRE ALARM SYSTEM.
10. **A FINAL ACCEPTANCE TEST SHALL BE CONDUCTED WITH AN INERT GAS.**
11. **NO SYSTEM SHALL BE PUT INTO SERVICE UNTIL THE FINAL ACCEPTANCE TEST AND INSPECTION ARE COMPLETE.**
12. **FINAL ACCEPTANCE TEST SHALL BE WITNESSED BY THE FIRE DEPARTMENT. AT THE TIME OF THE FINAL, THE SYSTEM AND ALL DEVICES WILL BE TESTED. PERSONS NECESSARY TO RESET THESE DEVICES NEED TO BE PRESENT FOR THE FINAL. TO SCHEDULE A TEST, CONTACT (651) 552-4172.**